**Data Transmission**

|  |  |
| --- | --- |
| **Q** | **Answer** |
| 1 | The payload contains the actual data being sent in the packet. • The trailer is a way of identifying the end of a packet and it also contains an error checking method, such as a cyclic redundancy check (CRC). |
| 2 | • The 500 KiB file is split up into a number of packets. • Each packet will follow its own path from 'A' to 'B'. • Routers (R1 to R10) will determine the path of each data packet. • The routing selection depends on the number of packets (at each router). • The shortest path available is always selected. |
| 3 | Three from: • There is no need to tie up a single communications line. • It is possible to overcome failed, busy or faulty lines by re-routing packets. • It is relatively easy to expand package usage. • A high data transmission rate is possible. |
| 4a | Four from: − Multiple bits are sent at the same time − Uses multiple wires − Data is sent in both directions … − … but only one direction at a time |
| b | Any two from: − Bits may arrive skewed − More expensive to setup/manufacture/purchase cable − Limited distance − More prone to interference/error |