|  |  |  |
| --- | --- | --- |
| 1 | LCD monitorLaser printer | 11 |
| 2 | Bar code readerOptical Character Reader | 11 |
| 3 | Four from:Products can be customised easily on requestSpeed of producing the product is faster than making it by handCheaper than making it by hand due to labour costsParts of equipment that are no longer made can be printed without having tomanufacture themMany copies of the original can be madeSaves the original from damage in transitCreate a fragile object from more robust materials**Refer ICT textbook edition 3, page number 23**  | 4 |
| 4 ab | Three from:ButtonsTouch screenMicrophoneCameraThree from:Speaker/headphoneTouch screenLED bulbBuzzer | 33 |
| 5 | Disadvantages:Maximum five from:A dot matrix printer is noisier when it prints therefore would not be used in anofficePrinting is slower using a dot matrixDot matrix prints line by line, whereas a laser is a page printerDot matrix printers cannot easily handle large print jobs, whereas laser printerscanPrinter ribbon is more expensive that tonerA dot matrix has more limited colour facilities as it uses a ribbonPrint quality is lower than a laser printerAdvantages:A dot matrix printer can be used is harsh conditionsA dot matrix uses a ribbon and ink which is far safer than toner which gives offozoneA dot matrix uses multipart stationery therefore carbon copies can be made asit printsCan use continuous stationery therefore less chance of the paper running outduring a print job | 6 |