**Quiz**

 **Marking Scheme**

**Data Transmission**

|  |  |  |
| --- | --- | --- |
| **Question** | **Description** | **Marks** |
| **1**  | Any three from: A packet is split into three different sections… the header … the payload … the trailer | **3** |
| **2**  | Router  | **1** |
| **3**  | Packet | **1** |
| **4**  | Each answer will get 1 markIP address of the sourceIP address of the receiverSequence number of the packetSize of the packet | **4** |
| **5** | The Actual data | **1** |