**Quiz**

**Marking Scheme**

**Data Transmission**

|  |  |  |
| --- | --- | --- |
| **Question** | **Description** | **Marks** |
| **1** | Any three from:  A packet is split into three different sections  … the header  … the payload  … the trailer | **3** |
| **2** | Router | **1** |
| **3** | Packet | **1** |
| **4** | Each answer will get 1 mark  IP address of the source  IP address of the receiver  Sequence number of the packet  Size of the packet | **4** |
| **5** | The Actual data | **1** |